**(LETTERHEAD)**

**CERTIFICATE OF COMPLIANCE OF VEHICLE SWEPT PATH PERFORMANCE**

**PROVIDING EXEMPTION FROM THE TRAVEL RESTRICTIONS FOR AN OVERDIMENSION VEHICLE**

**Background**

Land Transport Rule Vehicle Dimension and Mass 2002 (the Rule) specifies requirements for dimension and mass limits for vehicles operating on New Zealand roads. The Rule sets in place a regulatory regime so that vehicles are operated safely.

The Rule includes requirements for overdimension vehicles, including travel restrictions for overdimension vehicles as a method to manage the risk to public safety. The Rule also recognises that with appropriate design, an overdimension vehicle can be configured to perform cornering manoeuvres and use no greater road space than a maximum size standard vehicle. Therefore, the Rule provides facility for the road space requirements (swept path) of overdimension vehicles to be assessed and if appropriate, be exempt from the travel restrictions of the Rule.

**Certification**

Pursuant to section 6.6(11) of the Land Transport Rule Vehicle Dimensions and Mass 2002 Rule 41001 (the Rule) and by way of an approval from the New Zealand Transport Agency dated the …. day of (month) (year), I (Certifier), of (Company), verifies the following vehicle meets the specifications of Schedule 8 of the Rule. Therefore, subject to the conditions below the vehicle is granted exemption from the travel time requirements in Clause 6.12(3) of the Rule.

**Conditions:**

1. This Certificate shall be rendered void and of no effect if there are any changes to the vehicle that would result in it failing to meet the swept path requirements of Schedule 8 of the Rule or if the attached vehicle specifications are not complied with.
2. If the vehicle is traveling along a road whereby it cannot remain on the left hand side of the centreline road markings, or centre of the road if no centreline present, then this exemption will be invalid and the travel restrictions prescribed in the Rule for a Category 1 vehicle shall apply.
3. This Certificate shall be carried inside the cab of the vehicle at all times and shall upon request be presented to a Police Officer.
4. The operator of this vehicle must comply with all other Acts, regulations and laws pertaining to this vehicle.
5. This Certificate is revocable and shall forthwith be returned to the Director of the NZ Transport Agency on receipt of written notification to that effect form the Director.

Registration Number(s) of vehicle certified: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Certificate Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**Vehicle specifications:**

Number of Axles: Vehicle One:\_\_\_\_\_\_\_\_\_ Vehicle Two: \_\_\_\_\_\_\_\_\_\_\_\_

Tyre sizes: Vehicle One: \_\_\_\_\_\_\_\_\_ Front: \_\_\_\_\_\_\_\_\_ Rear: \_\_\_\_\_\_\_\_\_

Vehicle Two: \_\_\_\_\_\_\_\_\_ Front: \_\_\_\_\_\_\_\_\_ Rear: \_\_\_\_\_\_\_\_\_

*and any other relevant information to effecting vehicle’s ability to comply with Schedule 8 of the rule*

* *include dimensioned drawing of vehicle(s)*

Vehicle sketch with dimensions

Vehicle Specifications

Truck 🞏; Truck/trailer 🞏; Tractor/semi trailer 🞏; Grader 🞏; Truck Crane 🞏;

Trailing Boom Crane 🞏; Other 🞏;

Number of axles and configuration; Vehicle 1 \_\_\_\_\_\_\_\_\_\_ Vehicle 2 \_\_\_\_\_\_\_\_\_\_ Vehicle 3 \_\_\_\_\_\_\_\_\_

Location of steering axles; Vehicle 1 \_\_\_\_\_\_\_\_\_\_ Vehicle 2 \_\_\_\_\_\_\_\_\_\_ Vehicle 3 \_\_\_\_\_\_\_\_\_

Tyre sizes; Vehicle 1 \_\_\_\_\_\_\_\_\_\_ Vehicle 2 \_\_\_\_\_\_\_\_\_\_ Vehicle 3 \_\_\_\_\_\_\_\_\_

Additional conditions affecting compliance with Schedule 8/ Schedule 9 of the Rule;

Special operating conditions;

Inspected by: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ ID Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

Signed: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

***Print on the obverse of the Certificate of Compliance for Swept Path Performance***